*A proposal for*

***County of Rockland***

*5/15/2019*

**Western Star 4700SF**



Components shown may not reflect all spec'd options and are not to scale

## SPECIFICATION PROPOSAL

|  | | **Data Code** | | **Description** | | **Weight Front** | | **Weight Rear** | |  | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Price Level** | | | | | | | | | | |
|  | PRL-16T | | WESTERN STAR 4700 PRL-16T (EFF:04/25/17) | |  | |  | |  | | |
| **Data Version** | | | | | | | | | | |
|  | DRL-018 | | SPECPRO21 DATA RELEASE VER 018 | |  | |  | |  | | |
| **Vehicle Configuration** | | | | | | | | | | |
|  | 001-450 | | 4700 SET-FORWARD FRONT AXLE CHASSIS | | 9,100 | | 6,720 | |  | | |
|  | 004-218 | | 2018 MODEL YEAR SPECIFIED | |  | |  | |  | | |
|  | 002-001 | | SET FORWARD AXLE - TRACTOR | | 40 | |  | |  | | |
|  | 003-001 | | LH PRIMARY STEERING LOCATION | |  | |  | |  | | |
| **General Service** | | | | | | | | | | |
|  | AA1-001 | | TRACTOR/TRAILER CONFIGURATION | |  | |  | |  | | |
|  | AA6-001 | | DOMICILED, USA 50 STATES (INCLUDING CALIFORNIA AND CARB OPT-IN STATES) | |  | |  | |  | | |
|  | A85-011 | | CONSTRUCTION SERVICE | |  | |  | |  | | |
|  | A84-1GM | | GOVERNMENT BUSINESS SEGMENT | |  | |  | |  | | |
|  | AA4-002 | | LIQUID BULK COMMODITY | |  | |  | |  | | |
|  | AA5-002 | | TERRAIN/DUTY: 100% (ALL) OF THE TIME, IN TRANSIT, IS SPENT ON PAVED ROADS | |  | |  | |  | | |
|  | AB1-008 | | MAXIMUM 8% EXPECTED GRADE | |  | |  | |  | | |
|  | AB5-001 | | SMOOTH CONCRETE OR ASPHALT PAVEMENT - MOST SEVERE IN-TRANSIT (BETWEEN SITES) ROAD SURFACE | |  | |  | |  | | |
|  | 995-1A5 | | WESTERN STAR VOCATIONAL WARRANTY | |  | |  | |  | | |
|  | A66-99D | | EXPECTED FRONT AXLE(S) LOAD: 16000.0 lbs. | |  | |  | |  | | |
|  | A68-99D | | EXPECTED REAR DRIVE AXLE(S) LOAD: 46000.0 lbs. | |  | |  | |  | | |
|  | A63-99D | | EXPECTED GROSS VEHICLE WEIGHT CAPACITY: 62000.0 lbs. | |  | |  | |  | | |
|  | A70-99D | | EXPECTED GROSS COMBINATION WEIGHT: 107,000.0 lbs. | |  | |  | |  | | |
| **Tractor Service** | | | | | | | | | | |
|  | AA2-003 | | TANK TRAILER | |  | |  | |  | | |
|  | AH6-001 | | SINGLE (1) TRAILER | |  | |  | |  | | |
| **Engine** | | | | | | | | | | |
|  | 101-2YB | | DETROIT DD13 12.8L 470 HP @ 1625 RPM, 1900 GOV RPM, 1650 LB/FT @ 975 RPM | |  | |  | |  | | |
| **Electronic Parameters** | | | | | | | | | | |
|  | 79A-068 | | 68 MPH ROAD SPEED LIMIT | |  | |  | |  | | |
|  | 79B-000 | | CRUISE CONTROL SPEED LIMIT SAME AS ROAD SPEED LIMIT | |  | |  | |  | | |
|  | 79G-008 | | 10 MINUTES IDLE SHUTDOWN WITH CLUTCH AND SERVICE BRAKE OVERRIDE | |  | |  | |  | | |
|  | 79K-011 | | PTO MODE ENGINE RPM LIMIT - 1400 RPM | |  | |  | |  | | |
|  | 79M-002 | | PTO MODE BRAKE OVERRIDE - SERVICE BRAKE APPLIED, OR PARK BRAKE NOT APPLIED | |  | |  | |  | | |
|  | 79P-002 | | PTO RPM WITH CRUISE SET SWITCH - 700 RPM | |  | |  | |  | | |
|  | 79Q-003 | | PTO RPM WITH CRUISE RESUME SWITCH - 800 RPM | |  | |  | |  | | |
|  | 79T-001 | | PTO MODE RPM INCREMENT - 25 RPM | |  | |  | |  | | |
|  | 79U-007 | | PTO GOVERNOR RAMP RATE - 250 RPM PER SECOND | |  | |  | |  | | |
|  | 79W-001 | | ONE REMOTE PTO SPEED | |  | |  | |  | | |
|  | 79X-005 | | REMOTE PTO SPEED 1 SETTING - 900 RPM | |  | |  | |  | | |
|  | 80D-001 | | SOFT CRUISE CONTROL ENABLED | |  | |  | |  | | |
|  | 80G-001 | | PTO MINIMUM RPM - 600 | |  | |  | |  | | |
|  | 80L-001 | | ENABLE AUTO ENGINE RPM ELEVATE FOR EXTENDED IDLE | |  | |  | |  | | |
| **Engine Equipment** | | | | | | | | | | |
|  | 99C-017 | | 2016 ONBOARD DIAGNOSTICS/2010 EPA/CARB/FINAL GHG17 CONFIGURATION | |  | |  | |  | | |
|  | 99D-011 | | 2008 CARB EMISSION CERTIFICATION - CLEAN IDLE (INCLUDES 6X4 INCH LABEL ON LOWER FORWARD CORNER OF DRIVER DOOR) | |  | |  | |  | | |
|  | PMT-998 | | NO 2013 ENGINE ESCALATOR | |  | |  | |  | | |
|  | 13E-001 | | STANDARD OIL PAN | |  | |  | |  | | |
|  | 105-001 | | ENGINE MOUNTED OIL CHECK AND FILL | |  | |  | |  | | |
|  | 133-004 | | ONE PIECE VALVE COVER | |  | |  | |  | | |
|  | 014-1B5 | | SIDE OF HOOD AIR INTAKE WITH DONALDSON HIGH CAPACITY AIR CLEANER WITH SAFETY ELEMENT, FIREWALL MOUNTED | |  | |  | |  | | |
|  | 124-1D7 | | DR 12V 160 AMP 28-SI QUADRAMOUNT PAD ALTERNATOR WITH REMOTE BATTERY VOLT SENSE | |  | |  | |  | | |
|  | 292-071 | | (3) ALLIANCE MODEL 1231, GROUP 31, 12 VOLT MAINTENANCE FREE 3375 CCA THREADED STUD BATTERIES | | -10 | |  | |  | | |
|  | 290-1CD | | BATTERY BOX WITH ALUMINUM COVER MOUNTED SHORT SIDE TO RAIL | | 45 | | 10 | |  | | |
|  | 282-003 | | SINGLE BATTERY BOX FRAME MOUNTED LH SIDE BACK OF CAB | |  | |  | |  | | |
|  | 291-017 | | WIRE GROUND RETURN FOR BATTERY CABLES WITH ADDITIONAL FRAME GROUND RETURN | |  | |  | |  | | |
|  | 289-012 | | NON-POLISHED DIAMOND PLATE BATTERY BOX COVER | |  | |  | |  | | |
|  | 293-058 | | POSITIVE LOAD DISCONNECT WITH CAB MOUNTED CONTROL SWITCH MOUNTED OUTBOARD DRIVER SEAT | | 8 | |  | |  | | |
|  | 295-029 | | POSITIVE AND NEGATIVE POSTS FOR JUMPSTART LOCATED ON FRAME NEXT TO STARTER | | 2 | |  | |  | | |
|  | 107-044 | | BW MODEL BA-921 19.0 CFM SINGLE CYLINDER AIR COMPRESSOR WITH SAFETY VALVE | |  | |  | |  | | |
|  | 131-013 | | AIR COMPRESSOR DISCHARGE LINE | |  | |  | |  | | |
|  | 152-041 | | ELECTRONIC ENGINE INTEGRAL SHUTDOWN PROTECTION SYSTEM | |  | |  | |  | | |
|  | 128-002 | | JACOBS COMPRESSION BRAKE | |  | |  | |  | | |
|  | 016-1C2 | | RH OUTBOARD UNDER STEP MOUNTED HORIZONTAL AFTERTREATMENT SYSTEM ASSEMBLY WITH RH B-PILLAR MOUNTED VERTICAL TAILPIPE | |  | |  | |  | | |
|  | 28F-002 | | ENGINE AFTERTREATMENT DEVICE, AUTOMATIC OVER THE ROAD REGENERATION AND DASH MOUNTED REGENERATION REQUEST SWITCH | |  | |  | |  | | |
|  | 239-032 | | 11 FOOT 00 INCH (132 INCH+0/-5.9 INCH) EXHAUST SYSTEM HEIGHT | |  | |  | |  | | |
|  | 233-017 | | STANDARD CURVE BRIGHT UPPER STACK(S) | |  | |  | |  | | |
|  | 237-1CR | | RH CURVED VERTICAL TAILPIPE B-PILLAR MOUNTED ROUTED FROM STEP | |  | |  | |  | | |
|  | 23U-002 | | 13 GALLON DIESEL EXHAUST FLUID TANK | | 35 | | 10 | |  | | |
|  | 30N-003 | | 100 PERCENT DIESEL EXHAUST FLUID FILL | |  | |  | |  | | |
|  | 23Y-001 | | STANDARD DIESEL EXHAUST FLUID PUMP MOUNTING | |  | |  | |  | | |
|  | 23Z-002 | | NON-POLISHED ALUMINUM DIESEL EXHAUST FLUID TANK COVER | | 20 | | 10 | |  | | |
|  | 43X-002 | | LH MEDIUM DUTY STANDARD DIESEL EXHAUST FLUID TANK LOCATION | |  | |  | |  | | |
|  | 242-001 | | STAINLESS STEEL AFTERTREATMENT DEVICE/MUFFLER/TAILPIPE SHIELD | |  | |  | |  | | |
|  | 273-048 | | HORTON 2-SPEED DRIVEMASTER ADVANTAGE POLAREXTREME FAN DRIVE | |  | |  | |  | | |
|  | 276-002 | | AUTOMATIC FAN CONTROL WITH DASH SWITCH AND INDICATOR LIGHT, NON-ENGINE MOUNTED | |  | |  | |  | | |
|  | 110-068 | | DDC SUPPLIED ENGINE MOUNTED FUEL FILTER/FUEL WATER SEPARATOR WITH WATER-IN-FUEL INDICATOR | |  | |  | |  | | |
|  | 118-001 | | FULL FLOW OIL FILTER | |  | |  | |  | | |
|  | 266-057 | | 1500 SQUARE INCH ALUMINUM RADIATOR | |  | |  | |  | | |
|  | 267-006 | | MOUNTING FOR FIREWALL MOUNTED SURGE TANK | |  | |  | |  | | |
|  | 103-039 | | ANTIFREEZE TO -34F, OAT (NITRITE AND SILICATE FREE) EXTENDED LIFE COOLANT | |  | |  | |  | | |
|  | 171-007 | | GATES BLUE STRIPE COOLANT HOSES OR EQUIVALENT | |  | |  | |  | | |
|  | 172-001 | | CONSTANT TENSION HOSE CLAMPS FOR COOLANT HOSES | |  | |  | |  | | |
|  | 270-023 | | HDEP FIXED RATIO COOLANT PUMP AND RADIATOR DRAIN VALVE | |  | |  | |  | | |
|  | 168-998 | | NO RADIATOR/OIL PAN GUARD | | -5 | |  | |  | | |
|  | 138-005 | | PHILLIPS-TEMRO 1500 WATT/115 VOLT BLOCK HEATER | |  | |  | |  | | |
|  | 166-998 | | NO OIL PREHEATER | |  | |  | |  | | |
|  | 140-022 | | CHROME ENGINE HEATER RECEPTACLE MOUNTED UNDER LH DOOR | |  | |  | |  | | |
|  | 134-001 | | ALUMINUM FLYWHEEL HOUSING | |  | |  | |  | | |
|  | 155-074 | | DELCO 12V MOD 3.175-39MT+ OCP STARTER WITH THERMAL PROTECTION AND INTEGRATED MAGNETIC SWITCH | |  | |  | |  | | |
| **Transmission** | | | | | | | | | | |
|  | 342-1M1 | | ALLISON 4000 RDS AUTOMATIC TRANSMISSION WITH PTO PROVISION | | 170 | | 50 | |  | | |
| **Transmission Equipment** | | | | | | | | | | |
|  | 343-339 | | ALLISON VOCATIONAL PACKAGE 223 - AVAILABLE ON 3000/4000 PRODUCT FAMILIES WITH VOCATIONAL MODELS RDS, HS, MH AND TRV | |  | |  | |  | | |
|  | 84B-012 | | ALLISON VOCATIONAL RATING FOR ON/OFF HIGHWAY APPLICATIONS AVAILABLE WITH ALL PRODUCT FAMILIES | |  | |  | |  | | |
|  | 84C-023 | | PRIMARY MODE GEARS, LOWEST GEAR 1, START GEAR 1, HIGHEST GEAR 6, AVAILABLE FOR 3000/4000 PRODUCT FAMILIES ONLY | |  | |  | |  | | |
|  | 84D-023 | | SECONDARY MODE GEARS, LOWEST GEAR 1, START GEAR 1, HIGHEST GEAR 6, AVAILABLE FOR 3000/4000 PRODUCT FAMILIES ONLY | |  | |  | |  | | |
|  | 84E-013 | | S1 PREFORMANCE PRIMARY SHIFT SCHEDULE, AVAILABLE FOR 3000/4000 PRODUCT FAMILIES ONLY | |  | |  | |  | | |
|  | 84F-012 | | S1 PERFORMANCE SECONDARY SHIFT SCHEDULE, AVAILABLE FOR 3000/4000 PRODUCT FAMILIES ONLY | |  | |  | |  | | |
|  | 84G-009 | | 1800 RPM PRIMARY MODE SHIFT SPEED | |  | |  | |  | | |
|  | 84H-009 | | 1800 RPM SECONDARY MODE SHIFT SPEED | |  | |  | |  | | |
|  | 84L-010 | | DISABLE - LOAD BASED SHIFT SCHEDULE, DISABLE - VEHICLE ACCELERATION CONTROL | |  | |  | |  | | |
|  | 34C-010 | | ELECTRONIC TRANSMISSION CUSTOMER ACCESS CONNECTOR, BLUNT CUT, MOUNTED BETWEEN DRIVER AND PASSENGER SEATS | |  | |  | |  | | |
|  | 362-035 | | CUSTOMER INSTALLED CHELSEA 277 SERIES PTO | |  | |  | |  | | |
|  | 363-001 | | PTO MOUNTING, LH SIDE OF MAIN TRANSMISSION | |  | |  | |  | | |
|  | 341-018 | | MAGNETIC PLUGS, ENGINE DRAIN, TRANSMISSION DRAIN, AXLE(S) FILL AND DRAIN | |  | |  | |  | | |
|  | 345-003 | | PUSH BUTTON ELECTRONIC SHIFT CONTROL, DASH MOUNTED | |  | |  | |  | | |
|  | 97G-004 | | TRANSMISSION PROGNOSTICS - ENABLED 2013 | |  | |  | |  | | |
|  | 370-011 | | WATER TO OIL TRANSMISSION COOLER, FRAME MOUNTED | | 15 | |  | |  | | |
|  | 346-003 | | TRANSMISSION OIL CHECK AND FILL WITH ELECTRONIC OIL LEVEL CHECK | |  | |  | |  | | |
|  | 35T-001 | | SYNTHETIC TRANSMISSION FLUID (TES-295 COMPLIANT) | |  | |  | |  | | |
| **Front Axle and Equipment** | | | | | | | | | | |
|  | 400-1A9 | | DETROIT DA-F-16.0-5 16,000# FL1 71.0 KPI/3.74 DROP SINGLE FRONT AXLE | |  | |  | |  | | |
|  | 402-083 | | BENDIX ADB22X-V AIR DISC FRONT BRAKES | | 68 | |  | |  | | |
|  | 403-043 | | 2011/2013-FMVSS 121 RSD FRONT BRAKE LINING | |  | |  | |  | | |
|  | 419-004 | | FRONT DISC BRAKE ROTORS | |  | |  | |  | | |
|  | 427-001 | | FRONT BRAKE DUST SHIELDS | | 5 | |  | |  | | |
|  | 409-006 | | FRONT OIL SEALS | |  | |  | |  | | |
|  | 408-001 | | VENTED FRONT HUB CAPS WITH WINDOW, CENTER AND SIDE PLUGS - OIL | |  | |  | |  | | |
|  | 416-022 | | STANDARD SPINDLE NUTS FOR ALL AXLES | |  | |  | |  | | |
|  | 405-030 | | FRONT AIR DISC BRAKE INTERNAL ADJUSTERS | |  | |  | |  | | |
|  | 406-001 | | STANDARD KING PIN BUSHINGS | |  | |  | |  | | |
|  | 536-055 | | TRW THP-60 POWER STEERING WITH RCH45 AUXILIARY GEAR | | 90 | |  | |  | | |
|  | 539-003 | | POWER STEERING PUMP | |  | |  | |  | | |
|  | 534-003 | | 4 QUART POWER STEERING RESERVOIR | |  | |  | |  | | |
|  | 533-001 | | OIL/AIR POWER STEERING COOLER | |  | |  | |  | | |
|  | 40T-002 | | SYNTHETIC 75W-90 FRONT AXLE LUBE | |  | |  | |  | | |
| **Front Suspension** | | | | | | | | | | |
|  | 620-026 | | 16,000# TAPERLEAF FRONT SUSPENSION | | -100 | |  | |  | | |
|  | 619-004 | | GRAPHITE BRONZE BUSHINGS WITH SEALS - FRONT SUSPENSION | |  | |  | |  | | |
|  | 410-001 | | FRONT SHOCK ABSORBERS | |  | |  | |  | | |
| **Rear Axle and Equipment** | | | | | | | | | | |
|  | 420-111 | | RT-46-160P 46,000# R-SERIES TANDEM REAR AXLE | |  | | 450 | |  | | |
|  | 421-456 | | 5.38 REAR AXLE RATIO | |  | |  | |  | | |
|  | 424-001 | | IRON REAR AXLE CARRIER WITH STANDARD AXLE HOUSING | |  | | -30 | |  | | |
|  | 386-075 | | MXL 18T MERITOR EXTENDED LUBE MAIN DRIVELINE WITH HALF ROUND YOKES | |  | |  | |  | | |
|  | 388-073 | | MXL 17T MERITOR EXTENDED LUBE INTERAXLE DRIVELINE WITH HALF ROUND YOKES | |  | |  | |  | | |
|  | 452-006 | | DRIVER CONTROLLED TRACTION DIFFERENTIAL - BOTH TANDEM REAR AXLES | |  | | 30 | |  | | |
|  | 878-023 | | (1) INTERAXLE LOCK VALVE, (1) DRIVER CONTROLLED DIFFERENTIAL LOCK FORWARD-REAR AND REAR-REAR AXLE VALVE | |  | |  | |  | | |
|  | 87A-005 | | INDICATOR LIGHT FOR EACH INTERAXLE LOCKOUT SWITCH | |  | |  | |  | | |
|  | 87B-008 | | INDICATOR LIGHT FOR EACH DRIVER CONTROLLED TRACTION DEVICE SWITCH | |  | |  | |  | | |
| N | 423-1AD | | BENDIX 16.5X8.62X ES HEAVY DUTY SPIDER CAM REAR BRAKES, SINGLE ANCHOR | |  | |  | |  | | |
|  | 433-043 | | 2011/2013-FMVSS 121 RSD REAR BRAKE LININGS | |  | |  | |  | | |
|  | 434-003 | | STANDARD BRAKE CHAMBER LOCATION | |  | |  | |  | | |
|  | 451-023 | | CONMET CAST IRON REAR BRAKE DRUMS | |  | |  | |  | | |
|  | 440-006 | | REAR OIL SEALS | |  | |  | |  | | |
| \* | 426-1B3 | | BENDIX EVERSURE LONGSTROKE 2-DRIVE AXLES SPRING PARKING CHAMBERS | |  | |  | |  | | |
|  | 428-003 | | HALDEX AUTOMATIC REAR SLACK ADJUSTERS | |  | |  | |  | | |
|  | 41T-002 | | SYNTHETIC 75W-90 REAR AXLE LUBE | |  | |  | |  | | |
| **Rear Suspension** | | | | | | | | | | |
|  | 622-1H2 | | HENDRICKSON PRIMAAX EX 46,000# REAR AIR SUSPENSION | |  | | 420 | |  | | |
|  | 621-125 | | HENDRICKSON PRIMAAX 10.00" RIDE HEIGHT | |  | |  | |  | | |
|  | 431-003 | | AXLE CLAMPING GROUP | |  | |  | |  | | |
|  | 624-009 | | 54 INCH AXLE SPACING | |  | |  | |  | | |
|  | 888-048 | | MANUAL DUMP VALVE FOR AIR SUSPENSION WITH GAUGE | |  | |  | |  | | |
|  | 87D-006 | | INDICATOR LIGHT FOR EACH REAR SUSPENSION CONTROL SWITCH | |  | |  | |  | | |
|  | 910-001 | | SINGLE AIR REAR SUSPENSION LEVELING VALVE | |  | |  | |  | | |
|  | 623-002 | | TRANSVERSE CONTROL RODS | |  | |  | |  | | |
|  | 439-005 | | REAR SHOCK ABSORBERS - TWO AXLES (TANDEM) (AIR RIDE SUSPENSION) | |  | |  | |  | | |
| **Brake System** | | | | | | | | | | |
|  | 490-024 | | WABCO 6S/6M ABS WITHOUT TRACTION CONTROL | |  | |  | |  | | |
|  | 871-001 | | REINFORCED NYLON, FABRIC BRAID AND WIRE BRAID CHASSIS AIR LINES | |  | |  | |  | | |
|  | 904-001 | | FIBER BRAID PARKING BRAKE HOSE | |  | |  | |  | | |
|  | 412-001 | | STANDARD BRAKE SYSTEM VALVES | |  | |  | |  | | |
|  | 432-003 | | RELAY VALVE WITH 5-8 PSI CRACK PRESSURE, NO REAR PROPORTIONING VALVE | |  | |  | |  | | |
|  | 480-086 | | BW AD-9SI BRAKE LINE AIR DRYER WITH HEATER | |  | |  | |  | | |
|  | 483-003 | | BENDIX OIL COALESCING FILTER FOR AIR DRYER | |  | |  | |  | | |
|  | 479-005 | | AIR DRYER MOUNTED INBOARD ON RH RAIL | |  | |  | |  | | |
|  | 460-058 | | STEEL AIR TANKS MOUNTED AFT INSIDE AND/OR BELOW FRAME JUST FORWARD OF REAR SUSPENSION | |  | |  | |  | | |
|  | 477-001 | | PULL CABLE ON WET TANK, PETCOCK DRAIN VALVES ON ALL OTHER AIR TANKS | |  | |  | |  | | |
| **Trailer Connections** | | | | | | | | | | |
| \* | 481-998 | | NO TRAILER AIR HOSE | |  | |  | |  | | |
|  | 476-046 | | 49.5 INCH STAINLESS STEEL SLIDE BAR WITH SPRING TYPE AIR HOSE HANGER | | 2 | |  | |  | | |
|  | 484-006 | | COMBINATION DUMMY GLAD HANDS AND LIGHT PLUG HOLDER | |  | |  | |  | | |
|  | 296-010 | | PRIMARY CONNECTOR/RECEPTACLE WIRED FOR SEPARATE STOP/TURN, ABS CENTER PIN POWERED THROUGH IGNITION | |  | |  | |  | | |
|  | 297-005 | | SAE J560 7-WAY PRIMARY TRAILER CABLE RECEPTACLE FRAME MOUNTED AFT CAB | |  | |  | |  | | |
|  | 310-998 | | NO TRAILER ELECTRICAL CABLE | |  | |  | |  | | |
| **Wheelbase & Frame** | | | | | | | | | | |
| \* | 545-482 | | 4825MM (190 INCH) WHEELBASE | |  | |  | |  | | |
|  | 546-102 | | 7/16X3-9/16X11-1/8 INCH STEEL FRAME (11.11MMX282.6MM/0.437X11.13 INCH) 120KSI | | 160 | | 120 | |  | | |
|  | 552-017 | | 1475MM (58 INCH) REAR FRAME OVERHANG | |  | |  | |  | | |
|  | 55W-005 | | FRAME OVERHANG RANGE: 51 INCH TO 60 INCH | | 10 | | -50 | |  | | |
|  | AC8-99D | | CALC'D BACK OF CAB TO REAR SUSP C/L (CA) : 108.78 in | |  | |  | |  | | |
|  | AE8-99D | | CALCULATED EFFECTIVE BACK OF CAB TO REAR SUSPENSION C/L (CA) : 104.78 in | |  | |  | |  | | |
|  | AE4-99D | | CALC'D FRAME LENGTH - OVERALL: 264.97 | |  | |  | |  | | |
|  | AM6-99D | | CALC'D SPACE AVAILABLE FOR DECKPLATE : 73.04 in | |  | |  | |  | | |
| N | FSS-0LH | | CALCULATED FRAME SPACE LH SIDE : -29.4 in | |  | |  | |  | | |
|  | FSS-0RH | | CALCULATED FRAME SPACE RH SIDE : 72.09 in | |  | |  | |  | | |
|  | 553-002 | | FLANGED TAPERED END OF FRAME | |  | |  | |  | | |
|  | 559-001 | | STANDARD WEIGHT ENGINE CROSSMEMBER | |  | |  | |  | | |
|  | 561-001 | | STANDARD CROSSMEMBER BACK OF TRANSMISSION | |  | |  | |  | | |
|  | 562-001 | | STANDARD MIDSHIP #1 CROSSMEMBER(S) | |  | |  | |  | | |
|  | 572-020 | | INVERTED U TRACTOR CROSSMEMBER | |  | | 10 | |  | | |
|  | 565-002 | | HEAVY DUTY SUSPENSION CROSSMEMBER | |  | |  | |  | | |
|  | 568-001 | | STANDARD WEIGHT REAR SUSPENSION CROSSMEMBER | |  | |  | |  | | |
| **Chassis Equipment** | | | | | | | | | | |
|  | 674-019 | | LH BACK OF CAB ACCESS, GRAB HANDLES WITH SINGLE RUBBER INSERT | | 5 | | 5 | |  | | |
|  | 592-054 | | 21 INCH (525MM) DECK PLATE FLUSH MOUNTED BETWEEN RAILS | | 8 | | 7 | |  | | |
|  | 556-1AJ | | 16.5 INCH PLAIN ALUMINUM STRAIGHT BUMPER | | -70 | |  | |  | | |
|  | 558-033 | | REMOVABLE FRONT TOW HOOKS STORED ON THE CHASSIS FRAME | | 25 | |  | |  | | |
|  | 574-001 | | BUMPER MOUNTING FOR SINGLE LICENSE PLATE | |  | |  | |  | | |
|  | 585-1AH | | BETTS B-7 PAINTED MUDFLAP BRACKETS | |  | | 25 | |  | | |
|  | 590-032 | | WESTERN STAR LOGO BLACK MUDFLAPS | |  | | 15 | |  | | |
|  | 586-015 | | FRONT ANTI-SPRAY CAB MOUNTED MUDFLAPS | |  | |  | |  | | |
|  | 551-007 | | GRADE 8 THREADED HEX HEADED FRAME FASTENERS | |  | |  | |  | | |
|  | 44Z-001 | | EXTERIOR HARNESSES WRAPPED IN CONDUIT | |  | |  | |  | | |
| **Fifth Wheel** | | | | | | | | | | |
|  | 578-1T9 | | FONTAINE NO-SLACK II 7000 SERIES 7LWB 24.0 INCH AIR SLIDE FIFTH WHEEL WITH CAST TOP PLATE - 2 INCH SLIDE INCREMENTS | | 30 | | 500 | |  | | |
|  | 577-508 | | FIFTH WHEEL 508MM (20.0 INCHES) AHEAD OF SUSPENSION CENTERLINE | |  | |  | |  | | |
|  | 582-007 | | 184MM (7.25 INCH) FIFTH WHEEL HEIGHT | |  | |  | |  | | |
|  | 570-001 | | OUTBOARD ANGLE - FIFTH WHEEL MOUNTING | |  | |  | |  | | |
|  | 890-001 | | DASH MOUNTED CONTROL VALVE AND PLUMBING FOR FIFTH WHEEL | |  | |  | |  | | |
|  | 579-003 | | SIDE LEFT FIFTH WHEEL RELEASE | |  | |  | |  | | |
| **Fuel Tanks** | | | | | | | | | | |
|  | 204-156 | | 100 GALLON/378 LITER ALUMINUM FUEL TANK - LH | | 20 | |  | |  | | |
|  | 218-006 | | 25 INCH DIAMETER FUEL TANK(S) | |  | |  | |  | | |
|  | 215-007 | | PLAIN ALUMINUM/PAINTED STEEL FUEL/HYDRAULIC TANK(S) WITH POLISHED STAINLESS STEEL BANDS | |  | |  | |  | | |
|  | 212-007 | | FUEL TANK(S) FORWARD | |  | |  | |  | | |
|  | 664-001 | | PLAIN STEP FINISH | |  | |  | |  | | |
|  | 205-002 | | CHROME FUEL TANK CAP(S) | |  | |  | |  | | |
|  | 122-1K4 | | DAVCO 487 FUEL/WATER SEPARATOR WITH ESOC AND 12 VOLT PREHEATER | | 15 | |  | |  | | |
|  | 216-020 | | EQUIFLO INBOARD FUEL SYSTEM | |  | |  | |  | | |
|  | 202-016 | | HIGH TEMPERATURE REINFORCED NYLON FUEL LINE | |  | |  | |  | | |
|  | 221-998 | | NO FUEL COOLER | | -10 | |  | |  | | |
| **Tires** | | | | | | | | | | |
| \* | 093-2GV | | CONTINENTAL HTC1 425/65R22.5 20 PLY RADIAL FRONT TIRES | | 172 | |  | |  | | |
| \* | 094-2FK | | CONTINENTAL HDR2 12R22.5 16 PLY RADIAL REAR TIRES | |  | | 200 | |  | | |
| **Hubs** | | | | | | | | | | |
|  | 418-060 | | CONMET PRESET PLUS PREMIUM IRON FRONT HUBS | |  | |  | |  | | |
| \* | 450-060 | | CONMET PRESET PLUS PREMIUM IRON REAR HUBS | |  | |  | |  | | |
| **Wheels** | | | | | | | | | | |
|  | 502-1H5 | | ALCOA LVL ONE 82462X 22.5X12.25 10-HUB PILOT 4.68 INSET 10-HAND ALUMINUM DISC FRONT WHEELS | | -8 | |  | |  | | |
| \* | 505-1BH | | ACCURIDE 29169 22.5X8.25 10-HUB PILOT 5-HAND HD STEEL DISC REAR WHEELS | |  | | 328 | |  | | |
|  | 524-001 | | POLISHED FRONT WHEELS; OUTSIDE ONLY | |  | |  | |  | | |
|  | 496-011 | | FRONT WHEEL MOUNTING NUTS | |  | |  | |  | | |
|  | 497-011 | | REAR WHEEL MOUNTING NUTS | |  | |  | |  | | |
|  | 498-011 | | NYLON WHEEL GUARDS FRONT AND REAR ALL INTERFACES | |  | |  | |  | | |
| **Cab Exterior** | | | | | | | | | | |
|  | 829-1A8 | | 110 INCH BBC STEEL CONVENTIONAL CAB | |  | |  | |  | | |
|  | 82A-008 | | WESTERN STAR STAINLESS STEEL CAB SKIRT | |  | |  | |  | | |
|  | 650-044 | | AIR CAB MOUNTS WITH CHECK VALVE | |  | |  | |  | | |
|  | 705-007 | | STAINLESS STEEL SILL PLATES | | 5 | |  | |  | | |
|  | 648-002 | | NONREMOVABLE BUGSCREEN MOUNTED BEHIND GRILLE | |  | |  | |  | | |
|  | 667-001 | | FRONT FENDERS | |  | |  | |  | | |
|  | 754-001 | | 2 INCH FENDER EXTENSIONS | | 5 | |  | |  | | |
|  | 678-034 | | LH AND RH EXTERIOR GRAB HANDLES WITH RUBBER INSERTS AND RH INTERIOR GRAB HANDLE MOUNTED TO A POST | |  | |  | |  | | |
|  | 646-008 | | STATIONARY BRIGHT FINISH GRILLE | |  | |  | |  | | |
|  | 65X-003 | | CHROME HOOD MOUNTED AIR INTAKE GRILLE | |  | |  | |  | | |
|  | 640-008 | | GALVANEALED STEEL SEVERE SERVICE CAB | |  | |  | |  | | |
|  | 644-004 | | FIBERGLASS HOOD | |  | |  | |  | | |
|  | 690-007 | | HOOD LINER INSULATION WITH SINGLE FIREWALL INSULATION | |  | |  | |  | | |
|  | 727-019 | | SINGLE HADLEY SD-978 26 INCH RECTANGULAR AIR HORN | | -4 | |  | |  | | |
|  | 726-001 | | SINGLE ELECTRIC HORN | |  | |  | |  | | |
|  | 728-001 | | SINGLE HORN SHIELD | |  | |  | |  | | |
|  | 657-1AF | | DOORS AND IGNITION KEYED THE SAME (3 KEYS) | |  | |  | |  | | |
|  | 575-001 | | REAR LICENSE PLATE MOUNT END OF FRAME | |  | |  | |  | | |
|  | 327-012 | | SWITCH, INDICATOR LIGHT AND WIRING FOR (2) CUSTOMER FURNISHED BEACONS | |  | |  | |  | | |
|  | 312-072 | | SINGLE RECTANGULAR SEALED BEAM HEADLIGHTS WITH BRIGHT BEZELS | |  | |  | |  | | |
|  | 302-022 | | LED MARKER LAMPS | |  | |  | |  | | |
|  | 315-013 | | PERLUX 500SRS RECTANGULAR FOG LIGHTS IN BUMPER WITH AMBER LENS AND BLACK HOUSING | | 6 | |  | |  | | |
|  | 311-001 | | DAYTIME RUNNING LIGHTS | |  | |  | |  | | |
|  | 294-1AX | | INDIVIDUAL LED STOP/TURN/BACKUP LIGHTS GROMMET MOUNTED OUTBOARD OF RAIL | |  | | 5 | |  | | |
|  | 300-015 | | STANDARD FRONT TURN SIGNAL LAMPS | |  | |  | |  | | |
|  | 318-1D7 | | (2) FLUSH LED UTILITY LIGHTS MOUNTED BACK OF CAB/SLEEPER | | 6 | |  | |  | | |
|  | 744-1DH | | DUAL MEKRA AERO BRIGHT FINISH HEATED DUAL AXIS 1-PIECE MOTORIZED MIRRORS WITH LIGHTS, LH AND RH REMOTE AND INTEGRAL CONVEX MIRRORS | | 20 | |  | |  | | |
|  | 797-002 | | CAB MOUNTED MIRRORS | |  | |  | |  | | |
|  | 796-001 | | 102 INCH EQUIPMENT WIDTH | |  | |  | |  | | |
|  | 743-1AX | | DUAL MEKRA BRIGHT FINISH HEATED CONVEX MIRRORS WITH MANUAL ADJUSTMENT AND DUAL AXIS FOR 1-PIECE PRIMARY MIRRORS | |  | |  | |  | | |
|  | 74A-001 | | RH DOWN VIEW MIRROR | |  | |  | |  | | |
|  | 74B-014 | | RH AND LH VELVAC 8 INCH BRIGHT FINISH HOOD MOUNTED CONVEX MIRRORS WITH SWING ARM BRACKETS, DUAL VIEW | | 8 | |  | |  | | |
|  | 729-002 | | ADDITIONAL REFLECTORS BACK OF CAB/SLEEPER | |  | |  | |  | | |
|  | 73A-002 | | REAR REFLECTIVE DEVICE | |  | |  | |  | | |
|  | 787-020 | | ELECTRIC DOOR LOCKS, MECHANICAL KEY TUMBLER | |  | |  | |  | | |
|  | 677-054 | | RH AFTERTREATMENT SYSTEM CAB ACCESS WITH PLAIN DIAMOND PLATE COVER | |  | |  | |  | | |
|  | 764-002 | | STAINLESS STEEL EXTERIOR SUN VISOR | | 28 | |  | |  | | |
|  | 768-046 | | 17.5X35 INCH TINTED REAR WINDOW | |  | |  | |  | | |
|  | 661-006 | | TINTED DOOR GLASS | |  | |  | |  | | |
|  | 654-011 | | RH AND LH ELECTRIC POWERED WINDOWS | | 4 | |  | |  | | |
|  | 769-002 | | LOWER RH DOOR WINDOW WITH FRESNEL LENS | | 7 | |  | |  | | |
|  | 663-002 | | 2-PIECE TINTED CURVED GASKET MOUNTED WINDSHIELD | |  | |  | |  | | |
|  | 659-025 | | 2 GALLON WINDSHIELD WASHER RESERVOIR WITHOUT FLUID LEVEL INDICATOR, MOUNTED UNDER CAB, WITH REMOTE FILL | |  | |  | |  | | |
| **Cab Interior** | | | | | | | | | | |
|  | 707-1D0 | | GRAY VINYL BASE INTERIOR | |  | |  | |  | | |
|  | 70K-006 | | GREY HARD TRIM | |  | |  | |  | | |
|  | 706-049 | | BASE LEFT HAND DOOR TRIM | |  | |  | |  | | |
|  | 708-049 | | BASE RIGHT HAND DOOR TRIM | |  | |  | |  | | |
|  | 772-007 | | BLACK MATS WITH DOUBLE INSULATION | |  | |  | |  | | |
|  | 785-007 | | DASH MOUNTED ASH TRAY AND LIGHTER, DRIVER SIDE | |  | |  | |  | | |
|  | 691-001 | | FORWARD ROOF MOUNTED CONSOLE | |  | |  | |  | | |
|  | 694-009 | | PASSENGER SIDE WING DASH MOUNTED GLOVE BOX WITH LOCKING DOOR | |  | |  | |  | | |
|  | 697-012 | | 14"X7.75" DOCUMENT POUCH MOUNTED ON BACK WALL BETWEEN SEATS | |  | |  | |  | | |
|  | 693-025 | | LH AND RH DOOR MAP POCKETS | |  | |  | |  | | |
|  | 741-015 | | (2) COAT HOOKS ON BACKWALL OF CAB | |  | |  | |  | | |
|  | 742-026 | | (1) CUP HOLDER MOUNTED IN BOTTOM CENTER OF DASH | |  | |  | |  | | |
|  | 680-033 | | BLACK SOFT TOUCH WING DASH WITH DRIVER SIDE COSMETIC UNDER DASH COVER | |  | |  | |  | | |
|  | 320-004 | | STANDARD WIRING | |  | |  | |  | | |
|  | 720-003 | | 5 LB. FIRE EXTINGUISHER | | 10 | |  | |  | | |
|  | 700-023 | | HEATER, DEFROSTER AND AIR CONDITIONER WITH CONSTANT TEMPERATURE CONTROL AND COSMETIC COVER | |  | |  | |  | | |
|  | 701-010 | | HVAC DUCTING WITH FOAM MAIN FRESH AIR FILTER AND OUTSIDE PRE-FILTER | |  | |  | |  | | |
|  | 703-005 | | MAIN HVAC CONTROLS WITH RECIRCULATION SWITCH | |  | |  | |  | | |
|  | 170-015 | | STANDARD HEATER PLUMBING | |  | |  | |  | | |
|  | 130-033 | | DENSO HEAVY DUTY AIR CONDITIONER COMPRESSOR | |  | |  | |  | | |
|  | 698-001 | | RADIATOR MOUNTED AIR CONDITIONER CONDENSER | |  | |  | |  | | |
|  | 702-002 | | BINARY CONTROL, R-134A | |  | |  | |  | | |
|  | 739-001 | | CAB INSULATION | |  | |  | |  | | |
|  | 285-019 | | AUTOMATIC SELF-RESET CIRCUIT BREAKER IN MAIN DASH POWER DISTRIBUTION BOX AND CIRCUIT BREAKER/FUSE IN AUXILIARY POWER DISTRIBUTION BOXES | |  | |  | |  | | |
|  | 324-076 | | DOOR ACTIVATED DOME LIGHT, UNDER DASH LIGHT WITH LH AND RH DOOR MOUNTED COURTESY LIGHTS AND LH AND RH READING LIGHTS | |  | |  | |  | | |
|  | 655-005 | | LH AND RH ELECTRIC DOOR LOCKS | |  | |  | |  | | |
|  | 284-023 | | (1) 12 VOLT POWER SUPPLY IN DASH | |  | |  | |  | | |
|  | 722-028 | | TRIANGULAR REFLECTORS KIT WITHOUT FLARES SHIPPED LOOSE IN CAB | | 10 | |  | |  | | |
|  | 756-1DD | | BASIC HIGH BACK AIR SUSPENSION DRIVER SEAT WITH 1 CHAMBER AIR LUMBAR, INTEGRATED CUSHION EXTENSION AND REAR CUSHION TILT | |  | |  | |  | | |
|  | 760-1J2 | | BASIC HIGH BACK NON SUSPENSION TOOL BOX PASSENGER SEAT | |  | |  | |  | | |
|  | 759-009 | | INBOARD DRIVER SEAT ARMREST, NO PASSENGER SEAT ARMREST | | 2 | |  | |  | | |
|  | 758-022 | | BLACK MORDURA CLOTH DRIVER SEAT COVER | |  | |  | |  | | |
|  | 761-014 | | BLACK CORDURA PLUS CLOTH PASSENGER SEAT COVER | |  | |  | |  | | |
|  | 763-003 | | 3 POINT DRIVER AND PASSENGER SEAT BELT RETRACTORS | |  | |  | |  | | |
|  | 725-998 | | NO SUPPLEMENTAL RESTRAINT SYSTEM | |  | |  | |  | | |
|  | 532-002 | | ADJUSTABLE TILT AND TELESCOPING STEERING COLUMN | |  | |  | |  | | |
|  | 540-020 | | 2-SPOKE 18 INCH (450MM) BLACK STEERING WHEEL(S) | |  | |  | |  | | |
|  | 765-002 | | DRIVER AND PASSENGER INTERIOR SUN VISORS | |  | |  | |  | | |
| **Instruments & Controls** | | | | | | | | | | |
|  | 185-002 | | NON-ADJUSTABLE SUSPENDED PEDALS | |  | |  | |  | | |
|  | 870-005 | | STAR GAUGES WITH BRIGHT BEZELS | |  | |  | |  | | |
|  | 732-018 | | ROYAL ROSEWOOD MATTE FINISH DRIVER INSTRUMENT PANEL | |  | |  | |  | | |
|  | 734-017 | | ROSEWOOD VINYL MATTE FINISH CENTER INSTRUMENT PANEL INSERT | |  | |  | |  | | |
|  | 486-001 | | LOW AIR PRESSURE INDICATOR LIGHT AND AUDIBLE ALARM | |  | |  | |  | | |
|  | 840-002 | | 2 INCH PRIMARY AND SECONDARY AIR PRESSURE GAUGES | |  | |  | |  | | |
|  | 198-002 | | INTAKE MOUNTED AIR RESTRICTION INDICATOR WITH GRADUATIONS | |  | |  | |  | | |
|  | 721-001 | | 97 DB BACKUP ALARM | |  | | 3 | |  | | |
|  | 149-012 | | CRUISE CONTROL SWITCHES IN THE CENTER PANEL | |  | |  | |  | | |
|  | 156-007 | | KEY OPERATED IGNITION SWITCH AND INTEGRAL START POSITION; 4 POSITION OFF/RUN/START/ACCESSORY | |  | |  | |  | | |
|  | 811-001 | | WARNING LAMP/LIGHT BAR DISPLAY, NON-DATA LINKED | |  | |  | |  | | |
|  | 160-038 | | HEAVY DUTY ONBOARD DIAGNOSTICS INTERFACE CONNECTOR LOCATED BELOW LH DASH | |  | |  | |  | | |
|  | 844-001 | | 2 INCH ELECTRIC FUEL GAUGE | |  | |  | |  | | |
|  | 845-011 | | FUEL FILTER RESTRICTION INDICATOR | |  | |  | |  | | |
|  | 148-085 | | EMISSIONS LIMITED IDLE ADJUST | |  | |  | |  | | |
|  | 856-001 | | ELECTRICAL ENGINE COOLANT TEMPERATURE GAUGE | |  | |  | |  | | |
|  | 854-001 | | ENGINE OIL TEMPERATURE GAUGE | |  | |  | |  | | |
|  | 864-001 | | 2 INCH TRANSMISSION OIL TEMPERATURE GAUGE | |  | |  | |  | | |
|  | 372-035 | | (1) DASH MOUNTED PTO SWITCH WITH INDICATOR LAMP | | 5 | |  | |  | | |
|  | 852-002 | | ELECTRIC ENGINE OIL PRESSURE GAUGE | |  | |  | |  | | |
|  | 746-115 | | AM/FM/WB WORLD TUNER RADIO WITH BLUETOOTH AND USB AND AUXILIARY INPUTS, J1939 | | 10 | |  | |  | | |
|  | 747-002 | | ROOF/OVERHEAD CONSOLE MOUNTED RADIO | |  | |  | |  | | |
|  | 750-004 | | (4) RADIO SPEAKERS IN CAB | |  | |  | |  | | |
|  | 748-040 | | POWER AND GROUND WIRING AND BRACKET FOR CUSTOMER FURNISHED COBRA 29 CB RADIO IN OVERHEAD CONSOLE | | 2 | |  | |  | | |
|  | 752-017 | | MULTI-BAND AM/FM/WB/CB LH MIRROR MOUNTED ANTENNA SYSTEM | |  | |  | |  | | |
|  | 810-042 | | ELECTRONIC MPH SPEEDOMETER WITH SECONDARY KPH SCALE, WITH ODOMETER | |  | |  | |  | | |
|  | 817-001 | | STANDARD VEHICLE SPEED SENSOR | |  | |  | |  | | |
|  | 812-001 | | ELECTRONIC 3000 RPM TACHOMETER | |  | |  | |  | | |
|  | 813-1B4 | | VT-HU CONNECTIVITY PLATFORM HARDWARE | |  | |  | |  | | |
|  | 8D1-002 | | 2 YEARS DETROIT CONNECT BASE PACKAGE (VIRTUAL TECHNICIAN, DETROIT CONNECT PORTAL ACCESS) FOR VT-HU CONNECTIVITY PLATFORM | |  | |  | |  | | |
|  | 8Z1-998 | | NO ZONAR SERVICES SELECTED | |  | |  | |  | | |
|  | 162-002 | | IGNITION SWITCH CONTROLLED ENGINE STOP | |  | |  | |  | | |
|  | 329-064 | | TWO IGNITION CONTROLLED EXTRA SWITCHES WITH INDICATOR LIGHT, 20 AMPS, WIRED BEHIND PASSENGER SEAT | |  | |  | |  | | |
|  | 482-001 | | BW TRACTOR PROTECTION VALVE | |  | |  | |  | | |
|  | 883-001 | | TRAILER HAND CONTROL BRAKE VALVE | |  | |  | |  | | |
|  | 836-001 | | 2 INCH VOLTMETER | |  | |  | |  | | |
|  | 660-008 | | SINGLE ELECTRIC WINDSHIELD WIPER MOTOR WITH DELAY | |  | |  | |  | | |
|  | 304-015 | | CAB/TRAILER MARKER LIGHT SWITCH WITH SEPARATE HEADLIGHT SWITCH | |  | |  | |  | | |
|  | 882-004 | | TWO VALVE PARKING BRAKE SYSTEM WITH WARNING INDICATOR | |  | |  | |  | | |
|  | 299-037 | | SELF CANCELING TURN SIGNAL SWITCH WITH INTEGRAL HEADLAMP DIMMER WITH BRAKE OVERRIDE | |  | |  | |  | | |
|  | 298-036 | | PACIFIC INSIGHT ELECTRONIC FLASHER | |  | |  | |  | | |
| **Design** | | | | | | | | | | |
|  | 065-000 | | PAINT: ONE SOLID COLOR | |  | |  | |  | | |
| **Color** | | | | | | | | | | |
|  | 980-7IA | | CAB COLOR A: L2065EB SCHOOL BUS YELLOW ELITE BC | |  | |  | |  | | |
|  | 96J-001 | | CAB INTERIOR PAINTED SAME AS CAB COLOR | |  | |  | |  | | |
|  | 986-020 | | BLACK, HIGH SOLIDS POLYURETHANE CHASSIS PAINT | |  | |  | |  | | |
|  | 966-972 | | POWDER WHITE (N0006EA) REAR WHEELS/RIMS (PKWHT21, TKWHT21, W, TW) | |  | |  | |  | | |
| **Certification / Compliance** | | | | | | | | | | |
|  | 996-001 | | U.S. FMVSS CERTIFICATION, EXCEPT SALES CABS AND GLIDER KITS | |  | |  | |  | | |
| **Secondary Factory Options** | | | | | | | | | | |
|  | 82D-998 | | NO PDI INSTALLED GRILLE/HOOD TRIM | |  | |  | |  | | |
|  | 999-003 | | FRONT AND/OR REAR TIRE WIDTH EXCEEDS 2.6M (102.4 INCHES); DEALER ADVISED AND ACCEPTS | |  | |  | |  | | |

|  |
| --- |
| **TOTAL VEHICLE SUMMARY** |

|  |  |  |  |
| --- | --- | --- | --- |
| **Weight Summary** | | | |
|  | **Weight**  **Front** | **Weight**  **Rear** | **Total**  **Weight** |
| Factory Weight+ | 9966 lbs | 8838 lbs | 18804 lbs |
|  |  |  |  |
| Total Weight+ | 9966 lbs | 8838 lbs | 18804 lbs |

(+) Weights shown are estimates only.

If weight is critical, contact Customer Application Engineering.